# Ackland-Jones analysis

This modifier implements a method for identifying common crystalline and other structures based on an analysis of the distribution of angles formed by the pairs of neighbors of a central atom. The method is known as Ackland-Jones bond-angle method [Ackland and Jones, Phys. Rev. B 73, 054104]. The algorithm assigns a structural type to each particle having a local environment that matches one of the known structures (FCC, BCC, HCP, icosahedral).

Caution

The Ackland-Jones method tends to produce a lot of false positive identifications when being applied to strongly distorted or amorphous structures. Please consider using one of the more robust and well-defined identification methods available in OVITO instead, e.g. Polyhedral template matching or Common neighbor analysis. The Ackland-Jones modifier has only been implemented in OVITO for the sake of completeness, not because it is a good structure identification algorithm.

## Modifier outputs

The modifier outputs the classification results as a new particle property named `Structure Type`. This information allows you to subsequently select particles of a certain structural type, e.g. using the Select type modifier. The structural type determined by the algorithm is encoded as an integer value:

> - 0 = Other, unknown coordination structure

> - 1 = FCC, face-centered cubic

> - 2 = HCP, hexagonal close-packed

> - 3 = BCC, body-centered cubic

> - 4 = ICO, icosahedral coordination

In addition, the modifier assigns colors to the particles (by setting the `Color` particle property) to indicate their computed structural type. The color representing each structural type can be customized by double-clicking the corresponding entry in the table or, permanently, in the application settings dialog.

Furthermore, the modifier emits global attributes to the data pipeline reporting the total number of particles matching each of the supported structural types. These attributes are named `AcklandJones.counts.XXX`, where XXX stands for the name of a structure. These analysis statistics may be exported using OVITO’s data export function or displayed as live information in the viewports using a text label.

Note

The modifier needs to see the complete set of input particles to perform the analysis. It should therefore be placed at the beginning of the data pipeline, preceding any modifiers that delete some of the particles.

The option Use only selected particles restricts the analysis to the currently selected particles. In this case, unselected particles will be ignored (as if they did not exist) and are all assigned the structure type “Other”. This option is useful if you want to identify defects in a crystal type not directly supported by the bond-angle analysis algorithm but having a sub-lattice that is supported.

## Alternatives

OVITO provides implementations of other structure identification methods, for instance the Common neighbor analysis, Identify diamond structure or Polyhedral template matching modifiers. Furthermore, the Centrosymmetry parameter modifier can be used to detect defects in crystal lattices.

See also

`ovito.modifiers.AcklandJonesModifier` (Python API)